DELHI POLLUTION CONTROL COMMITTEE
DEPARTMENT OF ENVIRONMENT: GOVT. OF NCT OF DELHI
5TH FLOOR: ISBT BUILDING: KASHMERE GATE: DELHI-6

F.No.DPCC/5(9)(2)/CT-06/1449-1450

Dated: 19/06/09 

To

Sub.:
Quotation for Electricity wiring & fitting in Room No. 574.


This office is in the process to renovate the room no. 574 at 5th floor, ISBT Bldg., Kashmere Gate, Delhi.  If you are interested you may send the quotation in a sealed cover superscribing “rates for Electricity wiring & fitting in Room No. 574” latest by 4.00 p.m. on ___________. Rate should be as per DSR. No quotation will be entertained other than DSR. Specification of the material of renovation work are as under:- 

1. Wiring for light point / exhaust fan point / call bell point with 1.5 sqmm FR PVC insulated copper conductor single core cable in surface / recessed PVC conduit, with Modular plate / suitable GI box and earthing the point with 1.5 sqmm FR PVC insulated copper single core cable etc. as required.

2. Wiring for light / power plug with 2x4 sqmm FR PVC insulated copper conductor single core cable in surface / recessed PVC conduit along with 1 No. 1 sqmm FR PVC insulated copper conductor single core cable for loop earthing as required.

3. Wiring for light / power plug with 4x4 sqmm FR PVC insulated copper conductor single core cable in surface / recessed PVC conduit along with 2 Nos. 1 sqmm FR PVC insulated copper conductor single core cable in surface / recessed PVC conduit as required.

4. Wiring for circuit / submain wiring alongwith earth wire with 1x1.5 sqmm of FR PVC insulated copper conductor single core cable in surface / recessed PVC conduit as required.

5. Supply / installation / testing and commissioning of prewired 3x3 watt same as Model No. FBS 300/236 PSHP with all accessories and CFL lamp directly on ceiling / hanging / wall i.e. connection with 1.5 sqmm PVC insulated copper conductor single core cable etc. as required of reputed company like Philips, Crompton.

6. Supply and fixing of fancy fitting in round shape suitable for CFL lamp with all accessories and 2 Nos. CFL lamp 15/18 watt including connection, testing etc. as required.

7. S/F of exhaust fac (300 mm) of approved make like Crompton, Bajaj, Orient etc.

8. S/F of 3 switches, 3 sockets 5 Amp with GI box modular type including connection, testing etc. as required.

9. S/F of 15 Amp switch x 15 Amp socket modular type with GI box including connection, testing etc. as required.

Member Secretary, DPCC has reserve all right to accept or reject any or all quotations.  Site may be inspected in any working day between 11.00 A.M. to 05.00 P.M. before submission of quotation.
                                                                                                                       Sd/-

(H. P. Meena)

Admn. Officer

Copy to:

1. Notice Board of DPCC.
2. Incharge (Computer):- with a request to place on DPCC websites.
