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E-TENDER NOTICE
For supply of One Noise Meter for use in DPCC Laboratory

A. As directed by competent authority it is informed that tenders are invited through E-Tender
platform  (http://govtprocurement.delhi.gov.in) from Indian manufacturers / suppliers / Indian
agents of Foreign Manufacturers for the supply of one Noise Meter for use in DPCC Laboratory as
per specification enclosed as Annexure-A.

B. DETAILS OF TENDER

a) Last date of submitting of Quotations - 20-04-2012 at 03.00 PM.
b) Opening of Technical / Financial Quotation :- 20-04-2012 at 4.00 PM

C. ELIGIBILITY CRITERIA

1. The vendor must submit Earnest Money Deposit (EMD) of Rs. 3,000/~ (Three Thousand only) in
the form of Demand Draft drawn in favour of Delhi Pollution Control Committee and payable at
Delhi.

2. The vendor must have registration certificate of VAT / TIN Number and will attach authenticated
copy of the same with the technical quotations failing which the quotation will not be entertained
and shall be rejected.

3. Technical documentation (printed product brochures and all technical leaflets, etc) to be attached
compulsorily with the technical offer / bids.

4. Foreign manufacturers cannot participate in the bidding process directly. Only Indian agents who
desire to quote directly on behalf of their foreign manufacturers / principals can participate in the
bidding process. Such Indian agents should be enlisted with the department of Expenditure,
through the Central Purchase Organization i.e. DGS&D, as per compulsory Enlistment Scheme of
the Department of Expenditure, Ministry of Finance, Govt. of India. A self attested copy of such
enlistment certificate with DGS&D shall be enclosed with the technical bid, without which the bid
shall be rejected.

TWO BID SYSTEMS TENDER

a) Technical Tender / Bid
b) Financial Tender / Bid

1. Sealed Technical Bids comprising of Earnest Money along with all documents &

\ certificates listed under “Eligibility Criteria” should reach in office of Delhi Pollution
Control Committee, 4th Floor, ISBT Bldg., Kashmere Gate, Delhi-110006 latest by 3.00

ﬁﬁ?ﬂ PM on 20.04.2012 and be dropped in quotation box placed at Enquiry Counter, failing
which tender shall be rejected. Only sealed Technical bids superscribing “Technical

\

oy \! quotation for Noise Meter”” will be accepted.
)
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  [image: image2.jpg]E. GENERAL TERMS AND CONDITIONS

1. The prices must be quoted inclusive of all taxes & statutory levies and charges i.e. basic price, taxes,
packing, forwarding & transportation charges, insurance, installation charges etc.

2. The quotations shall be submitted only in Indian rupees. The Indian agent will be legally
responsible to ensure the delivery of the goods as per specifications and along with all requite
documents.

3. One years onsite comprehensive warranty covering all parts & labours. This period will start from
the date of successful delivery / commissioning of the instrument.

4. The technical bids will be opened individually, and examined for short listing the vendors, and the
commercial / financial bids of only those vendors who have qualified technically will be opened and
compared.

5. DPCC at its discretion may extend the last date of submission of bids and opening of bids. The final
authority for acceptance of bids will rest with Competent Authority, DPCC who does not bind
himself to accept the lowest bids and is vested with the authority to reject and or all the bids received
without assigning any reason.

6. The instruments / equipments have to be supplied in standard packaging only to Dr. M. P. George,
Scientist-D, at Delhi Pollution Control Committee at 4" Floor, ISBT Bldg., Kashmere Gate, Delhi-
110006.

7. Instruments / equipments bearing ISI mark, CE certification & better specifications / features will be
given preference and priority.

8. The vendor must deliver the instrument within 30 — 45 days from the date of placement of orders. If
the vendor fails to deliver any or all the equipment for which tenders are invited, the EMD amount
may be forfeited.

9. If the equipments / instruments supplied are found defective / unsatisfactory condition / short supply
/ other than specifications in the purchase orders, the same will have to be replaced at the supplier’s
risk & cost. No freight & other charges will be paid by DPCC.

10. The specifications are clearly mentioned as above and the bidder are requested to submit Bid only if
their offer strictly comply to above specifications. Please note that no deviation in the required
specifications will be permitted. The bidding for instruments having different specification will be
on bidder’s risk as DPCC will not entertain such bids.

11. Any dispute arising out of this purchase shall be under the jurisdiction of the courts of Delhi.

12. The Competent Authority, DPCC reserves the right to reject any or all the tenders without assigning
any reason at any stage.

F. PAYMENT TERMS

1. 100 % payment will be released after recei pt of the instrument / equipment in good & satisfactory
condition and on installation / commissioning the instrument / equipment along with the related
papers (to be certified by the concerned officer i.e. Sr. Scientist (Lab.) DPCC and on submission
of bills in duplicate).

2. No advance payment shall be allowed in any case.

3. The payment shall be issued / released in the name of Indian agent only.

This issue with the approval of competent authority vide UO No. Secy (Env)/4478 dated
09.03.2012.
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ADMN. OFFICER

Copy to:-

\_k"8r. Scientist (IT):- with request to upload on DPCC website.
2. Enquiry Counter, DPCC.
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Specification of the Noise Level Meter:-

I- Should cover 20— 140 dBA
m Switchable to A, Linerar, Octave and 1/3 rd octave.
Min. IEC 804 (BS 6698) Grade I or ANS] Type I
m 0.1 dB over full range
_M Digital Leq. SPL, Liax and L, over a programmable Range.

6 Time Weighing Switchable to different time intervals i.e. 1/8 Sec, I Sec, 10 Sec.

ete. or slow, fast, Max.

[7 | Power Suppiy 1

8 Computer Interface Data logging system with RS 232 interface / USB

9 Calibration Automatic calibration

10 0’Cro55’C

11 M Sufficient memory to store atleast 24 hrs, Data for all parameters

|

given in modes and octave band analaysis,
1. Calibrator (See specification)

2. Tripod Stand

3. Wind Screen

4. Batteries

5. Carrying case of kit

Accessories Required

Specifications:-

1. Calibrator:-
i. Level (dB) - Atleast two one each in lower and higher range.
ii. Frequency = 1kHz
iii. Accuracy -+03dBat25°C
iv. Adaptors = 25mm, 12.5 mm, 6.25 mm

3. Further Details / information required:-

Leq in bytes.

Built in memory in bytes,

Whether data logger in built in the unit or is a separate system,

Details of software, in-built /spread sheet.

Whether the system is compatible for measurement of other parameters like meteorology.
Whether octave provided or not

a) If yes; its range.

& Whether the software has facility for:-

a) Retrieval of short leg elements.

Post processing to produce Leq and Ln measurements over any period automatic event detection
etc.
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