DELHI POLLUTION CONTROL COMMITTEE
DEPARTMENT OF ENVIRONMENT: GOVT. OF NCT OF DELHI
5TH FLOOR: ISBT BUILDING: KASHMERE GATE: DELHI-6

F.No.DPCC/CT-2010/4616-17



Dated: 06-08-2010

Sub.:
Quotation for work of Aluminum Partition for Bacteriological Laboratory in DPCC at 4th Floor.

Sealed Quotations are invited for the work of Aluminum Partition for bacteriological  laboratory in DPCC at 4th floor.  There are provisions of 03 cabins.    Specifications of the work are as under:-

	S. No.
	Description of Item
	Area (Sq./Mtr)
	Rates per sq/mtr

	1
	Providing & Fixing partition with Laminated Board (12.5 mm) of ISI mark / glass of specifies pattern (5 mm) with built up standard hollow section including all accessories.  Rates should be including of aluminium door, window, door closer and its fittings etc. i.e. complete in all respect.
	60.00
	

	2
	Providing and fixing at all height falls ceiling including providing and fixing of frame work made of special sections power pressed from MS sheet and galvanized in accordance with zinc coating of grade 350 as per IS:277 and consisting of angle cleats of size 25 mm wise X 1.6 mm thick with flanges of 22 mm and 37 mm at 12.00 mm centre to centre one flange fixed to the ceiling with dash fastner 12.5 mm dia X40 mm long with 6 mm centre to centre one flange fixed to the ceiling with dash fastner 12.5 mm dia X40 mm long with 6 mm dia bolts to the angle hangers of 25x25x0.55 mm of required length, and other end of angle hanger being fixed with nut & bolts to GI channels 45 X15X0.9 mm running at the rate of 1200 mm centre to centre to which the ceiling section 0.5 mm thick bottom wedge of 80 mm with tapered flanges of 26mm each having clips of 10.5 mm at 450 mm centre to centre shall be fixed in a direction perpendicular to GI channel with connecting clips made out of 2.64 mm dia X 230 mm long GI wire at every junction including fixing the gypsum board with ceiling section and perimeter channels 0.5 mm thick 27 mm high having flanges of 20 mm and 30 mm long, the perimeter of ceiling fixed to wall/partition with the help of raw plugs at 350 mm centre to centre with 25 mm long drive-all screws @ 230 mm interval including jointing and fixing to a flush finish of tapered and square edges of the board with recommended filler, jointing tapes, finisher and two coats of primer suitable for board as per manufactures specification and also including the cost of making openings for light fittings, grills, diffusers, cutouts made with frame of perimeter channels suitable fixed all complete as per drawing and specification and direction of the Engineer-in Charge but excluding the cost of painting.

With 12.5 mm thick tapered edge gypsum board conforming to IS: 2095-Part-I (ISI Mark)
	30.00
	

	3
	Distempering with oil bound washable distemper of approved brand (Nerolac/Asian) and manufacture to give an even shade.

a) New work (two or more coats) over and including priming coat with cement primer)
	30.00
	


 Sealed Quotations must reach in office of Delhi Pollution Control Committee, 4th Floor, ISBT Bldg., Kashmere Gate, Delhi-110006 latest by 3.30 PM on 16.08.2010 and be dropped in quotation box placed at Enquiry Counter.  Only sealed quotations superscribing “Quotation for Aluminium Partition for bacteriological laboratory in DPCC.” will be accepted. The agency must have valid TIN / Service Tax number and shall attach a copy of TIN / Service tax registration with the quotation.   M.S., DPCC reserves all right to reject or accept any or all quotations without assigning any reason.

This issue with the approval of competent authority vide UO No.MS/8615 dated 06.08.2010.
ADMINISTRATIVE OFFICER

Copy to:

1. Notice Board of DPCC.

2. Incharge (Computer):- with a request to place on DPCC websites.

