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Sub.: Quotation for Renovation of unsued space attached with Room No.
541 & 544 (CMC) at 5™ Floor, ISBT Bldg.,

Sealed quotations are invited for the renovation of unused space attached with room no. 541
& 544 (CMC) at 5" Floor, ISBT Bldg.  The sealed cover containing quotation whall be
super scribed on top of the envelop “rates for renovation of unsued space attached with room
no. 541 & 544 (CMC room)” latest by 4.00 p.m. on 06-11-09. Rate should be as per DSR. No
quotation will be entertained other than DSR. Specification of work / material of renovation
work are as under:-

S.No Description of Ttem Qty.

1 Dismantling stone slab flooring laid in cement mortar including stacking of | 410
serviceable material and disposal of unserviceable material within 50 meters lead. sq.mirs

2 Dismentling/Demolishing brick mzmually / by mechanical means including stacking | 14 Sq.
of serviceable material and disposal of unserviceable material within 50 meter lead. Mtrs.

3 Dismentling/Demolishing door window manually / by mechanical means including | 55 Sq.
stacking of serviceable material and disposal of unserviceable material within 50 | Murs
meter lead

4 Repair of Plaster etc. 58 Sq.

o Mirs

5 Fixing of Chowkhat including making opening etc. o 02 Nos.

6 Aluminum sliding door fitted with board & fittings etc | 02Nos

7 Polished vitrified floor tiles of make Kajaria or equivalent in different si (thickness | 74.48

to be specified by the manufacturer) with water absorptions less than 1% and flexural | sq.mirs
strength not less than 30 N/MM?, in colours and shades, size of tiles 60 x 60 cm, aid on
20 mm thick cement mortar 1:4 (1 cement : 4 coaurse sand) including grouting the
joints with white cement and matching pigments etc. complete.
8 medmg 2 mm thick POP on walls as per direction of Engineer-in-charge. 301 sq.mtrs|
9 Distempering with oil bound washable distemper of approved brand and manufacture | 301

to give an even shade sq.mtrs
a) New work (two or more coats) including priming coal with cement primer.

Member Secretary, DPCC has reserve all right to accept or reject any or all quotations
Site may be inspected in any working day between 11.00 AM. to 05.00 P.M. befor
submission of quotation.

Quotation must be reached in office at Enquiry Counter (quotation box) 4™ Floor, ISBT
Bldg., Kashmere Gate, Delhi-110006 latest by 4.00 PM on 10.10.2009. 4
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(S.P. MEENA

Admn. Office)
Copy to:

1. Notice Board of DPCC.
/Z/Incharge (Computer):- with a request to place on DPCC websites.





