DELHI POLLUTION CONTROL COMMITTEE
DEPARTMENT OF ENVIRONMENT: GOVT. OF NCT OF DELHI
5TH FLOOR: ISBT BUILDING: KASHMERE GATE: DELHI-6

F.No.DPCC/5(9)(2)/CT-06/2482

   Dated: 24-09-2009

Sub.:
Renovation of Room No. 575 at 5th Floor, ISBT Bldg.,


This office is in the process to renovate the Room no. 575 at 5th floor, ISBT Bldg. If you are interested you may send the quotation in a sealed cover super scribing “rates for renovation of room no. 575” latest by 3.00 p.m. on 09-10-09. Rate should be as per DSR. No quotation will be entertained other than DSR. Specification of the material of renovation work are as under:-

	S.No
	Description of Item
	Qty.

	1
	Providing & fixing aluminum work for door, windows, ventilators and partitions with ext4ruded built-up standard tubular sections/appropriate Z section and other sections of approved make conforming to IS”733 and IS: 1285 fixed with raw plugs and screws or with fixing clips, or with expansion hold fasters including necessary filling-up of gaps at junctions, at top, bottom and side with required PVC/neoprene flat etc.  Aluminum section shall be smooth, rust free, straight mitred and jointed mechanically wherever required including cleat angle, aluminum snap beading for glazing/paneling, CP brass/stainless steel screws, all complete as per architectural drawing and the directions of Engineer-in-Charge (Glazing and paneling to be paid for separately)

b) For shutters of door, windows & ventilators including providing and fixing hinges/pivots and making provision for fixing of fittings wherever required including the cost of PVC/neoprene gasket required (Fittings shall be paid for separately) Anodized aluminum (anodized transparent or dyed to required shade according to IS: 1868, minimum anodic coating of grade AC 15)
	11.78 sq.mtrs

	2
	Demolishing brick manually / by mechanical means including stacking of serviceable material and disposal of unserviceable material within 50 meter lead as per direction of Engineer-in-charge.  In cement mortar.
	2.30 Cu. Mts.

	3
	Providing and fixing at all height false ceiling including providing and fixing of frame work made of special sections power pressed f3rom MS sheet and galvanized in accordance with zinc coating of grade 350 as per IS:277 and consisting of angle cleats of size 25 mm wise X 1.6 mm thick with flanges of 22 mm and 37 mm at 12.00 mm centre to centre one flange fixed to the ceiling with dash fastner 12.5 mm dia X40 mm long with 6 mm centre to centre one flange fixed to the ceiling with dash fastner 12.5 mm dia X40 mm long with 6 mm dia bolts to the angle hangers of 25x25x0.55 mm of required length, and other end of angle hanger being fixed with nut & bolts to GI channels 45 X15X0.0 mm running at the rate of 1200 mm centre to centre to which the ceiling section 0.5 mm thick bottom wedge of 80 mm with tapered flanges of 26mm each having clips of 10.5 mm at 450 mm centre to centre shall be fixed in a direction perpendicular to GI channel with connecting clips made out of 2.64 mm dia X 230 mm long GI wire at every junction including fixing the gypsum board with ceiling section and perimeter channels 0.5 mm thick 27 mm high having flanges of 20 mm and 30 mm long, the perimeter of ceiling fixed to wall/partition with the help of raw plugs at 350 mm centre to centre with 25 mm long drive-all screws @ 230 mm interval including jointing and fixing to a flush finish of tapered and square edges of the board with recommended filler, jointing tapes, finisher and two coats of primer suitable for board as per manufactures specification and also including the ost of making openings f3or light fittings, grills, diffusers, cutouts made with frame of perimeter channels suitable fixed all complete as per drawing and specification and direction of the Engineer-in Charge but excluding the cost of painting.

With 12.5 mm thick tapered edge gypsum board conforming to IS: 2095-Part-I
	37.60 sq.mtrs

	4
	Polished vitrified floor tiles of make Kajaria or equivalent in different size (thickness to be specified by the manufacturer) with water absorptions less than 1% and flexural strength not less than 30 N/MM2, in colours and shades, size of tiles 60 x 60 cm, aid on 20 mm thick cement mortar 1:4 (1 cement : 4 coaurse sand) including grouting the joints with white cement and matching pigments etc. complete.

	37.60 sq.mtrs

	5
	Providing 2 mm thick POP on walls as per direction of Engineer-in-charge.
	80  sq.mtrs

	6
	Distempering with oil bound washable distemper of approved brand and manufacture to give an even shade
a) New work (two or more coats) including priming coal with cement primer.


	120  sq.mtrs

	7
	Providing and fixing venation blind for window (vertical) of approved brand and fixing in position etc. complete in all respect as per the direction Engineer-in-charge.
	6   sq.mtrs


	8
	Dismantling stone slab flooring laid in cement mortar including stacking of serviceable material and disposal of unserviceable material within 50 meters lead.
	14   sq.mtrs

	9
	Providing and fixing Ist quality ceramic glazed wall tiles conforming to IS: 15622 of minimum thickness 5 mm of approved make like NITCO, ORIENT, SOMANY KAJARIA or equivalent make in all colours, shades except begundy, bottle green, black of any size as approved by Engineer-in-change in skirting, risers of steps and dados over 12 mm thick bed of cement mortar 1: 3 (1 cement:3 coarse sand) and jointing with g4rey cement slurry @ 3.3. Kg per sqm including pointing in white cement mixed with pigment of matching shade complete.
	12   sq.mtrs

	10
	Providing & laying ceramic glazed floor tiles 300x300 mm (thickness to be specified by the manufacturer) of 1ist quality confirming to IS : 15622 of approved make in colours such as White, lvory, Grey, Fume Red Brown, laid on 20 mm thick cement mortal 1:4 (1 cement: 4 coarse sand including pinting the joints with white cement and matching pigments etc, complete.
	4    sq.mtrs

	11
	Providing and fixing white vitreous china pedestal type water closet (European type W.C. flushing cistern with manually controlled device (handle lever), conforming to IS: 7231, with all fittings, and fixtures complete including cutting and making good the walls and floors wherever required.

a) W.C. pan with ISI marked white solid plastic seat and lid.
	1 Nos

	12
	Providing and fixing wash basin with CI/MS brackets, 15 mm CP brass pillar taps, Kingston/Gem/Techno/Parko, 32 mm CP brass waste of standard pattern, including painting of fittings and brackets, cutting and making good the walls wherever required:

a) White Vitreous China flat back wash basin size 550x400 mm with single 15 mm CP brass pillar tapes
	1  Nos

	13
	Providing and fixing white vitreous china flat back or wall corner type lipped front urinal basin of 430 x260x350mm and 340x410x265mm sizes respectively with automatic flushing cistern with standard flush pipe and C.P. brass spreaders with brass unions and G.I. clamps complete, including painting of fittings and brackets, cutting and making good the walls and floors wherever required.

a) One urinal basin with 5 litre white PVC automatic flushing cistern.
	1  Nos

	14
	Providing and fixing brass bib cock of approved quality.

a) 15 mm nominal bore.
	1  Nos

	15
	Providing and fixing CP brass angle valve for basin mixer and gyser points of approved quality confirming to IS:8931.

a) 15 mm nominal bore.
	4  Nos

	16
	Providing and fixing unplasticised PVC connection pipe with brass unions.

a) 45 cm length – 15 mm nominal bore
	4  Nos

	17
	Providing and fixing trap of self cleansing design with screwed down or hinged grating with or without vent arm complete, including cost of cutting and making goods the walls and floor. A) 100 mm inlet and 100 mm outlet Sand cast iron S&S as per IS: 3989
	2  Nos

	18
	Providing and fixing soil, waste and vent pipes:

a) 100 x 100 x 100 mm Sand cast iron S & S as per IS-1729
	10  Mtr

	19
	Providing and fixing single equal plain junction of required degree:

a) 100x100x100mm Sand cast iron S & S as per IS-1729
	1  Nos

	20
	Prividing and fixing heel rest sanitary bend.

a) 100 mm dia.
	1  Nos

	21
	Concealed pipe including  painting with anti corrosive bit mastic paint, cutting chases and making good the wall”

a) 25 to 40 mm nominal bore
	10 Mtr

	22
	Extra for using colored pedestal type W.C. pan (European type) with low level cistern of same colour instead of white vitreous china W.C. pan and cistern.
	3 Nos


Member Secretary, DPCC has reserve all right to accept or reject any or all quotations.  Site may be inspected in any working day between 11.00 A.M. to 05.00 P.M. before submission of quotation.
(S.P. MEENA)

      Admn. Officer
Copy to:

1. Notice Board of DPCC.

2. Incharge (Computer):- with a request to place on DPCC websites.

