DELHI POLLUTION CONTROL COMMITTEE
DEPARTMENT OF ENVIRONMENT: GOVT. OF NCT OF DELHI
4TH FLOOR: ISBT BUILDING: KASHMERE GATE: DELHI-6


           





Dated: 10-07-09

To

Sub.:
Quotation for Tile flooring (Vitrified)


This office is in the process to renovate / repair laboratory (Area 140 sqm)  at 4th floor, ISBT Bldg., Kashmere Gate, Delhi.  Quotation in a sealed cover superscribing “rates for Repair / Renovation of laboratory” are invited latest by 17-07-2009. Rate should be as per DSR. No quotation will be entertained other than DSR. Specification of the material of renovation work area as under:-
1. Polished vitrified floor tiles of make Kajaria or equivalent in different size (thickness to be specified by the manufacturer) with water absorption less than 1% and flexural strength not less than 30 N/MM2 , in colours and shades, size of tiles 60 x 60 cm, aid on 20 mm thick cement mortar 1:4 (1 cement:4 coarse sand) including grouting the joints with white cement and matching pigments etc. complete.
   Member Secretary, DPCC has reserve all right to accept or reject any or all quotations.  Site may be inspected in any working day between 11.00 A.M. to 05.00 P.M. before submission of quotation.
Dr. Nandita Moitra









   (Sr. Scientist)

Copy to:

1. Notice Board of DPCC.

2. Incharge (Computer):- with a request to place on DPCC websites.

