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F.No.DPCC/12(3)34/Lab/2013//46 ¢ § Date:- 2 2 /, // y

E-TENDER NOTICE

A. As directed by competent authority it is informed that tenders are invited through E-Tender
platform (http://govtprocurement.delhi.gov.in) from Indian manufacturers / suppliers /
Indian agents of Foreign Manufacturers for the supply of following laboratory equipments
/ instruments as per specification enclosed as Annexure-A & B.

S.No. | Name of Laboratory instruments /| Quantity required | Specifications
equipments

1 PM 2.5 Sampler 02 Nos Annexure-A

2 RDS (PM,o) 04 Nos Annexure-B

B. DETAILS OF TENDER

a) Last date of submitting of Quotations - 27.02.2014 at 01.00 PM.
b) Opening of Technical / Financial Quotation :- 27-02-2014 at 04.00 PM

C. ELIGIBILITY CRITERIA

Following essential documents shall be attached with technical bids & submit
physically failing which tender shall be rejected.

1. The vendor must submit Earnest Money Deposit (EMD) of Rs. 50,000/ (Fifty Thousand only)
in the form of Demand Draft drawn in favour of Delhi Pollution Control Committee and
payable at Delhi and will upload scanned copy of the same on E-Tender Website
(http:/govtprocurement.delhi.gov.in) alongwith his quotations.

2. The vendor must have registration certificate of VAT / TIN Number issued by Govt. of Delhi.

3. Copy regarding specifications / technical documentation (printed product brochures and all
technical leaflets, etc).

4. Foreign manufacturers cannot participate in the bidding process directly. Only Indian agents
who desire to quote directly on behalf of their foreign manufacturers / principals can participate
in the bidding process. Such Indian agents should be enlisted with the department of
Expenditure, through the Central Purchase Organization i.e. DGS&D, as per compulsory
Enlistment Scheme of the Department of Expenditure, Ministry of Finance, Govt. of India. A
copy of such enlistment certificate with DGS&D shall be attached with technical quotations. In
absence of non-compliance of this provision, the quotations shall not entertained.

D. TWO BID SYSTEMS TENDER

a) Technical Tender / Bid
b) Financial Tender/ Bid

1. Sealed Technical Bids comprising of Earnest Money along with all documents & certificates
listed under “Eligibility Criteria” should reach in office of Delhi Pollution Control
Committee, 4th Floor, ISBT Bldg., Kashmere Gate, Delhi-110006 latest by 01.00 PM on
27.02.2014 and be dropped in quotation box placed at Enquiry Counter, failing which tender
shall be rejected. Only sealed Technical bids superscribing “Technical quotation for RDS

X & PM Samplers” will be accepted.
\Contd...Z

SeEaE \





[image: image2.jpg]10.

1.

12.

13.

14.
15

~

page 2 of 3

GENERAL TERMS AND CONDITIONS

. The prices quoted should be exclusive of all taxes, statutory levies, insurance and

installation charges.

The quotations shall be submitted only in Indian rupees. The Indian agent will be legally
responsible to ensure the delivery of the goods as per specifications and along with all
requite documents.

The approved agency shall ensure that Delivery of goods is made from Delhi and against a
sale invoice issued from Delhi. The dealer supplying goods should be registered with the
Delhi VAT Department and carry a valid tax identification number issued by it.

One years onsite comprehensive warranty covering all parts & labours. This period will
start from the date of successful delivery / commissioning of the instrument.

The technical bids will be opened individually, and examined for short listing the vendors,
and the commercial / financial bids of only those vendors who have qualified technically
will be opened and compared. :

The successful bidder shall have to deposit the performance security of an amount of ten
percent (10%) of the actual value of the contract and if any stage, the tender deviates from
the terms and conditions of such contract agreement or his performance is found to be
unsatisfactory, the contract agreement shall be liable to be terminated without any notice
and the performance security shall be forfeited.

DPCC at its discretion may extend the last date of submission of bids and opening of bids.
The final authority for acceptance of bids will rest with Competent Authority, DPCC who
does not bind himself to accept the lowest bids and is vested with the authority to reject and

or all the bids received without assigning any reason.

The instruments / equipments have to be supplied in standard packaging only to Dr. M. P.
George, Scientist-D, at Delhi Pollution Control Committee at 5" Floor, ISBT Bldg.,
Kashmere Gate, Delhi-110006.

Instruments / equipments bearing ISI mark, CE certification & better specifications /
features will be given preference and priority.

The instruments / equipments may increase or decrease as per discretion of competent
authority, DPCC.

The vendor must deliver the instrument within 30 — 45 days from the date of placement of
orders. If the vendor fails to deliver any or all the equipment for which tenders are invited, the
EMD amount may be forfeited.

If the equipments / instruments supplied are found defective / unsatisfactory condition / short
supply / other than specifications in the purchase orders, the same will have to be replaced at
the supplier’s risk & cost. No freight & other charges will be paid by DPCC.

The specifications are clearly mentioned as above and the bidder are requested to submit Bid
only if their offer strictly comply to above specifications. Please note that no deviation in the
required specifications will be permitted. The bidding for instruments having different
specification will be on bidder’s risk as DPCC will not entertain such bids.

Any dispute arising out of this purchase shall be under the jurisdiction of the courts of Delhi.
The Competent Authority, DPCC reserves the right to reject any or all the tenders without
assigning any reason at any stage.
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E: ARBITRATION

Any dispute arising out of this purchase shall be referred for settlement through
arbitration proceedings. Arbitration procedure will be as per Indian Arbitration and
Conciliation Act, 1996. The arbitrator will be appointed by the Lt. Governor, Delhi.

G FORCE MAJEURE

(a) Any delay or failure in the performance by either party hereunder shall be excused if and
to the extent caused by the occurrence of a Force Majeure. For purposes of this
agreement, Force majeure shall mean a cause or event that is not reasonably foreseeable
or otherwise caused by or under the control of the party claiming Force Majeure,
including acts of God, fires, floods, explosions, riots, wars, hurricane, sabotage terrorism,
vandalism, accident, restraint of government, governmental acts, injunctions, labor
strikes, other than those of seller or its supplier, that prevent seller from furnishing the
materials or equipment, and other like events that are beyond the reasonable anticipation
and control of the party affected thereby, despite such party’s reasonable efforts to
prevent, avoid, delay, or mitigate the effect of such acts, events or occurrences, and which
events or the effects thereof are not attributable to a party’s failure to perform its
obligations under this agreement.

(b) If a force majeure situation arises, the supplier shall promptly notify the DPCC in writing
of such conditions and the cause thereof. Unless otherwise directed by the DPCC in
writing, the contract as far as reasonably practical, shall seek all reasonable alternatives
means for performance not prevented by the force majeure event. Any of the parties may
terminate this contract, by giving a written notice of minimum thirty days to the other
party if as a result of force majeure, the other party being unable to perform its obligation
as per this contract for a period of more than sixty days.

H. PAYMENT TERMS

1. 100 % payment will be released after receipt of the instrument / equipment in good &
satisfactory condition and on installation / commissioning the instrument / equipment
along with the related papers (to be certified by the concerned officer i.e. Scientist-D
(Lab.) DPCC and on submission of bills in duplicate).

2. No advance payment shall be allowed in any case.

3. The payment shall be issued / released in the name of Indian agent only.

This issue with the approval of competent authority vide UO No. MS/3371 dated

21.01.2014.
@L‘l‘el\ ’L/

ADMN. OFFICER
Copy to:-

1. SEE (IT):- with request to upload on DPCC website.
2. Enquiry Counter, DPCC.
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DELHI POLLUTION CONTROL COMMITTEE
5" FLOOR ISBT BUILDING, KASHMERE GATE, DELHI-110006
(LABORATORY CELL)

Name of Laboratory Item/ Instrument/ Equipment to be procured:-

1. PM 2.5 SAMPLER.
2. RDS. (PM,g)

Specification:- Specification of PM 2.5 SAMPLER and RDS. (PM,g) is

enclosed herewith.
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%J) Signature of laboratory incharge
Secenhy B
Date :- Name & Designation
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SPECIFICATIONS of PM 2.5 SAMPLER [l b

Salient Features

Flow rate: Fixed 1 m%hour (16.7 Ipm) controlled by Mass Flow
Controller

Flow Meter: + 3% accuracy at 1 m¥/hour
Constant flow controller: + 5% accuracy in 1m3/hour
Elapsed time indicator: upto 9999 hours with two decimal.

Vacuum Pump: Diaphragm type, brush less induction motor with oil
free pump.

Flow recorder: Digital micro controller based.

Dry Gas meter (Volume Totaliser) : For measuring total volume of air
sampled.

Power requirement: 220 VAC = 10% 50 Hz 0.5 Amp. Max.
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Flow Rate: 0.9-1.4 m3/min free flow

Particle Size: A cyclone is used for fractionating the dust into fractions. D-
50 for the cyclone is at 10 microns. PM 10 dust is accumulated on the filter
paper while coarse dust is collected in a cup placed under the cyclone.
Sampling Time: 28 hours (maximum)

Sampling Time Record: 0-999.99 hrs recorded on a Time Totalizer.
Automatic Sampling: 24hrs programmable timer to automahcally shut off
the system after preset time interval.

Power requirement: Normal 220V, Single Phase 50 Hz AC mains supply.
Brushless with Electronic flow controller





