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/ \ DELHI POLLUTION CONTROL COMMITTEE .

s DEPARTMENT OF EN VIRONMENT: GOVT. OF NGT OF DELHI
4" & 5™ FLOOR: ISBT BUILDING: KASHMERE GATE: DELHI-6
F.No.DPCC/l2(3)26/Lab(N)/201 1/ 7}f> . ‘7 Date:- l‘?/////
TENDER NOTICE
For supply of One Noise Meter for use in DPCC Laboratory
A. As directed by competent authority it is informed that tenders are invited from Indian

manufacturers / suppliers / Indian agents of Foreign Manufacturers for the supply of one Noise
Meter for use in DPCC Laboratory as per specification enclosed as Annexure-A

B. DETAILS OF TENDER

a) Last date of submitting of Quotations - 15-12-2011 at 03.00 PM.
b) Opening of Technical / Financial Quotation = 15-12-2010 at 4.00 PM

C. ELIGIBILITY CRITERIA

1. The vendor must submit Earnest Money Deposit (EMD) of Rs. 3,000/- (Three Thousand only)
in the form of Demand Draft drawn in favour of Delhi Pollution Control Committee and
payable at Delhi.

2. The vendor must have registration certificate of VAT / TIN Number and will attach
authenticated copy of the same with the technical quotations failing which the quotation will
not be entertained and shal] be rejected.

3. Technical documentation (printed product brochures and all technical leaflets, etc) to be
attached compulsorily with the technical offer / bids.

4. Foreign manufacturers cannot participate in the bidding process directly. Only Indian agents

\ who desire to quote directly on behalf of their foreign manufacturers / principals can participate

in the bidding process. Such Indian agents should be enlisted with the department of

‘ Expenditure, through the Central Purchase Organization i.e. DGS&D, as per compulsory
\)%9 Enlistment Scheme of the Department of Expenditure, Ministry of Finance, Govt. of India. A

D. TWO BID SYSTEMS TENDER

a) Technical Tender/ Bid
b) Financial Tender / Bid

1. Sealed Technical quotation must comprise of documents as referred under “Eligibility
Criteria” above. The sealed envelope containing technical quotation should be superscribed
as “Technical quotation for Noise Meter”.

2. Sealed financial quotation comprising price of the “Noise Meter” shall be superscribed as
“Financial quotation for Noise Meter”. The prices must be quoted inclusive of all taxes
& statutory levies and charges ie. basic price, taxes, packing, forwarding &
transportation charges, insurance, installation charges etc.

3. Both the envelopes containing Technical Quotation and Financial Quotation shall be put in
outer envelope. The outer envelope should be sealed and superscribed as “Quotatation for
Noise Meter”. The quotation shall be addressed to Member Secretary, Delhi Pollution
Control Committee, 4% Floor, ISBT Building, Kashmere Gate, Delhi-110006 and shall
invariably be dropped in the sealed tender box at the enquiry counter, 4 Floor, ISBT
Building, Kashmere Gate, Delhi-110006.

The quotations not adhering with the above procedure shall be rejected
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1. The quotations shall be submitted only in Indian rupees. The Indian agent will be legally
responsible to ensure the delivery of the goods as per specifications and along with all requite
documents.

2. One years onsite comprehensive warranty covering all parts & labours. This period will start
from the date of successful delivery / commissioning of the instrument.

3. The technical bids will be opened individually, and examined for short listing the vendors,
and the commercial / financial bids of only those vendors who have qualified technically will
be opened and compared.

4. DPCC at its discretion may extend the last date of submission of bids and opening of bids.
The final authority for acceptance of bids will rest with Competent Authority, DPCC who
does not bind himself to accept the lowest bids and is vested with the authority to reject and
or all the bids received without assigning any reason.

5. The instruments / equipments have to be supplied in standard packaging only at Delhi
Pollution Control Committee at 4™ Floor, ISBT Bldg., Kashmere Gate, Delhi-110006.

6. Instruments / equipments bearing ISI mark, CE certification & better specifications / features
will be given preference and priority.

7. The vendor must deliver the instrument within 30 — 45 days from the date of placement of
orders. If the vendor fails to deliver any or all the equipment for which tenders are invited, the
EMD amount may be forfeited.

8. If the equipments / instruments supplied are found defective / unsatisfactory condition / short
supply / other than specifications in the purchase orders, the same will have to be replaced at
the supplier’s risk & cost. No freight & other charges will be paid by DPCC.

9. The specifications are clearly mentioned as above and the bidder are requested to submit Bid
only if their offer strictly comply to above specifications. Please note that no deviation in the
required specifications will be permitted. The bidding for instruments having different
specification will be on bidder’s risk as DPCC will not entertain such bids.

10. Any dispute arising out of this purchase shall be under the jurisdiction of the courts of Delhi.

I1. The Competent Authority, DPCC reserves the right to reject any or all the tenders without
assigning any reason at any stage.

F. PAYMENT TERMS

1. 100 % payment will be released after receipt of the instrument / equipment in good &
satisfactory condition and on installation / commissioning the instrument / equipment along
with the related papers (to be certified by the concerned officer i.e. Sr. Scientist (Lab.) DPCC
and on submission of bills in duplicate).

2. No advance payment shall be allowed in any case.

3. The payment shall be issued / released in the name of Indian agent only.

This issue with the approval of competent authority vide UO No. MS/1361 dated 24.11.2011.
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[image: image3.jpg]Specification of the Noise Level Meter:-

ANNEXURE-A

1 Measurement Range Should cover 20 — 140 dBA

2 Frequency Weighing Switchable to A, Linerar, Octave and 1/3 rd octave.

3 Accuracy Min. IEC 804 (BS 6698) Grade I or ANSI Type |

4 Resolution 0.1 dB over full range

= Display Digital Leq. SPL, Ly and Ly, over a programmable Range.

6 Time Weighing Switchable to different time intervals i.e. 1/8 Sec, I Sec, 10 Sec.
etc. or slow, fast, Max.

7 Power Supply Battery System

8 Computer Interface Data logging system with RS 232 interface / USB

9 Calibration Automatic calibration

10 Temperature 0°Cto55°C

11 Memory Sufficient memory to store atleast 24 hrs. Data for all parameters
given in modes and octave band analaysis.

Accessories Required 1. Calibrator (See specification)
2. Tripod Stand
3. Wind Screen
4. Batteries
5. Carrying case of kit

Specifications:-

1. Calibrator:-
i. Level (dB)
ii. Frequency
iii. Accuracy
iv. Adaptors

2. Data Logger:-

:- Atleast two one each in lower and higher range.
- 1 kHz

-+03dBat25°C

- 25 mm, 12.5 mm, 6.25 mm

Communications with data logger should be possible using a standard RS 232 / USB cable along
with compatible modems in order to provide communications facilities (Radio / Telephone).
The SBM compatible software supplied with the data logger shall be able to handle all
communications requirements.

3. Further Details / information required:-

Leq in bytes.

ol o SIS

a) If yes; its range.

Built in memory in bytes.

Whether data logger in built in the unit or is a separate system.

Details of software, in-built / spread sheet.

Whether the system is compatible for measurement of other parameters like meteorology.
Whether octave provided or not

g. Whether the software has facility for:-
a) Retrieval of short leg elements.
Post processing to produce Leq and Ln measurements over any period automatic event detection

etc.





