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Delhi Pollution Control Committee intends to undertake
a study for the assessment of :

e Ambient Air Quality for twenty four hours at 41 locations
simultaneously on monthly basis.

® Noise levels monitoring preferably for twenty four

hours, at above 41 locations simultaneously or in four
days on monthly basis.
Noise Monitoring shall be undertaken using Type-l,
Integrating Data Logging Noise Level Meters with
Applicable Standards.

1) IEC61672-1:2002 Class 1 or2 Group X

2) IEC60651:2001 Type 1 or Type 2

3) IEC60804:2000 Type 1 or Type 2

4) ANSI S1.4with NK: 70 Random Incidence Adaptor

1:1 & 1:3 Octave Filters to IEC 61260 Class 1
(where Fitted)

The interested agencies may collect details and
conditions of study from the office or download from the
website http://dpcc.delhigovt.nic.in. The offers shall be
submitted to this office on or before 15 April 2009, at 3:00
PM which will be opened, at 3:30 PM on the same day.

- Member Secretary
“orcc_  DELHI POLLUTION CONTROL COMMITTEE

“———__  Department of Environment, Govt. of NCT of Delhi
m 4" Floor, ISBT Building, Kashmere Gate, Delhi-6

“" Visit us at : http://dpcc.delhigovt.nic.in

20x16 = 80cc = 320 sqg.cm.





Terms & Conditions
1. Company shall start work of Ambient Air Monitoring for Parametrs of SPM, RSPM, SO2, NO2 and CO from April 2009 and Noise monitoring for parameters of Leq db(A) (Hourly, Day time &Night time  and for 24hours)  Ln99,Ln90, Ln50 ,Ln10, Lmax, Lmin and real time noise levels from June 2009, for financial year 2009-2010.

2. The Monitoring will be conducted by the Company on the days informed by the Committee for each month.

3. Monitoring is to be conducted by the Company strictly as per CPCB guidelines.

· The Respirable Suspended Particulate Matter (RSPM) and Suspended Particulate Matter (SPM) should be monitored using separate HVS & RDS.

· The Noise level should be assessed using Type – I Integrating Data Logging Noise Level Meters with Applicable Standards.

1) IEC 61672-1:2002 Class 1 or 2 Group X

2) IEC 60651:2001 Type 1 | or Type 2 |

3) IEC 60804:2000 Type 1 or Type 2

4) ANSI S1.4 with NK: 70 Random Incidence Adaptor

    1:1 & 1:3 Octave Filters to IEC 61260 Class 1(where Fitted)
4. The Equipments/ instruments used by the Company in this study shall be properly calibrated and calibration certificate must be made available to this office before start of the work.

5. The samples used by the Company shall be analyzed as per standard methods approved by CPCB and analyze and develop correlation and submit the report to Committee within subsequent two working days of each monitoring, including a graphic presentation. 

6. The Company shall ensure that its person  engaged for data collection/analyst be  maintain perfect discipline and behavior and they shall not in any manner cause any interference, annoyance, nuisance to the public or to the management of the Committee or its officials/ officers/ employees. 

7. This agreement will be for a period of one year from the date of execution of these presents. The Committee shall, in the event of the Company committing any breach of any of the terms and conditions of this agreement or if the services provided by the Company is considered to be unsatisfactory by the Committee or for any other reason considered by the Committee as insufficient, be entitled to terminate this agreement by giving one month's notice in writing and the Company shall not be entitled to any compensation in case of such termination.  
8. In case of failure in submission of the data within prescribed period, the Company will be liable to pay Rs. 3,000/- ( Three Thousand) for each day of delay to the Committee. 
9. If data collected by the Company is found substandard or in violation of CPCB Guidelines in collection/analysis by the Committee, penalty of Rs.50,000/(Rs. Fifty Thousand only) can be imposed after giving a opportunity to be heard. 

10.  Data generated out of the study is the property of the Committee and can not be supplied to third party or used by the Company in any form.
11. The offers shall be submitted in two parts technical and financial. The envelopes shall be clearly marked as “Offer for Ambient Air and Noise Monitoring at 41 locations in Delhi” and deposited in the tender box kept in the office of Delhi Pollution Control Committee 4th Floor I.S.B.T. Building Kashmiri Gate Delhi-6.

12. The publication of Notice inviting tender not binding to award the work, the Committee have all right to except or reject any or all offers.
