DELHI POLLUTION CONTROL COMMITTEE
DEPARTMENT OF ENVIRONMENT: GOVT. OF NCT OF DELHI
5TH FLOOR: ISBT BUILDING: KASHMERE GATE: DELHI-6

F.No.DPCC/5(9)(2)/CT-06/1447-1448
           
Dated: 19-06-09

To

Sub.:
Quotation for Repair / Renovation of Room No. 574.


This office is in the process to renovate / repair the room no. 574 at 5th floor, ISBT Bldg., Kashmere Gate, Delhi.  If you are interested you may send the quotation in a sealed cover superscribing “rates for Repair / Renovation of Room No. 574” latest by 4.00 p.m. on 29-06-2009. Rate should be as per DSR. No quotation will be entertained other than DSR. Specification of the material of renovation work is as under:- 

1. Plaster of paris putty works of 2mm thickness for smoothness of walls of 140 sqm. approx.

2. Providing and fixing at all height false ceiling including providing and fixing of frame work, fixing the gypsum of 12.5 mm thick board with ceiling section and perimeter channels, including jointing and fixing to a flush finish of tapered and square edge of board, two coats of primer suitable for board and also including the cost of making openings for light fittings, grills, diffusers, cutouts made with frame of perimeter channels suitably fixed all complete as per drawing / specification and direction of the DPCC but excluding the cost of painting.

3. Distempering with oil bound washable distemper of approved brand and manufacture to give an even shade including priming coal with cement primer.

4. Aluminum sliding door fitted with board & fittings etc.

Member Secretary, DPCC has reserve all right to accept or reject any or all quotations.  Site may be inspected in any working day between 11.00 A.M. to 05.00 P.M. before submission of quotation.
(M. C. Jain)

Sr. Account Officer

Copy to:

1. Notice Board of DPCC.

2. Incharge (Computer):- with a request to place on DPCC websites.

