[image: image1.jpg]DELHI POLLUTION CONTROL COMMITTEE
4" & 5™ FLOOR: ISBT BUILDING: KASHMERE GATE: DELHI-6
FNO.DPCC/5(3)2/CT/08/ 10 37§ -7 7 Date:- 1 ] LYo

Sub: Quotation for purchase of one “Mechanical Compactor” with complete installation in
DPCC office.

As directed it is informed that sealed quotations are invited for installation of one
“Mechanical Compactor” equivalent to 12 almirah / shelves [(3 bay X 4 row) or (2 bay X 6 row)
or (2 bay X 4 row)] with complete installation in DPCC office. Specifications of the mechanical
compactor are as under:-

Sl. | Specifications of Mechanical Compactor
No
1 Model:- Mechanical Three bay deep

Storage Units:-

1. Single faced Static / Fixed unit— 1980mm x 2745mm x 457 mm

2. Single face movable unit — 1980mm x 2745mm x 457 mm

3. Double faced movable unit — 1980mm x 2745mm x 914 mm

4. Overall height of compactor from ground level to compactor top panel —2130 mm (i.e.
1980mm body + 120mm base frame + 30 mm track & moving clearance).

5. Body — Body of quality pre-coated sheet of 0.8 mm thick with protective film, material
should confirm to IS 14246 class-3. Weldless multiple bends body with compete knock
down & inbuilt upright in front panel.

6. Shelves — Shelves in 10 fold for better strength & better load bearing capacity. Material
pre-coated sheet of 0.8 mm thickness with protective film.

Last Date for Submitting Quotation:- 14.09.2012 at 14.00 PM
Date of Opening Quotation: - 14.09.2012 at 16.00 PM

Terms & Conditions

1. Earnest Money of Rs. 1000/-(One Thousand only) in form of Demand Draft in favour Delhi Pollution
Control Committee.

2. The vendor must have registration certificate of VAT / TIN Number. Self Attested copy of VAT / TIN
No. shall attach.

3. Above document shall be kept in sealed envelope which shall be superscribed as “Technical
Quotations for Mechanical Compactor”. A technical quotations not accompanied with above
documents shall be rejected without any further communication in this regards.

4. Sealed financial quotation comprising price for Mechanical Compactor shall be superscribed as
“Financial Quotations for Mechanical Compactor”.

5. Both the envelopes containing Technial Quotation and Financial Quotation shall be put in outer
envelope. The outer envelope shall superscribed as Quotation for Mechanical Compactor and should
be addressed to Member Secretary, Delhi Pollution Control Committee, 4™ Floor, ISBT Building,
Kashmere Gate, Delhi-110006 and shall invariably be dropped in the sealed tender box at the enquiry
counter, 4" Floor, ISBT Building, Kashmere Gate, Delhi-110006 latest by 14.09.2012 at 02.00 PM.

6. The quotations not adhering with the above procedure shall be rejected.

Competent Authority, DPCC reserves all right to reject or accept any or all quotations without

assigning any reason
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This issues with the prior approval of the Competent Authority vide UO No. MS/2127 dated 28.08.2012.
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